**LBTR05F**

**5-port 10/100BASE-TX Industrial Ethernet Switch**

**Interface**

* 5-port 10/100Base-Tx RJ-45 with auto negotiation and auto-MDI/MDI-X function

**Industrial conformance**

* 12V to 52V DC, redundant power input
* -40℃ to 80℃ operating temperature
* IP40 Aluminum housing
* Supports 6KV DC Ethernet ESD protection
* Supports 6KV DC EFT protection for power line
* Free Fall, Shock and Vibration Stability
* DIN-rail and wall-mountable hardware design

**Slim Type with more Practicability and Convenience**

LBTR05F an hardened 5-port Industrial Ethernet Switch, provides non-blocking wire-speed performance in harsh industrial environment. It also provides 5-port 10/100/100BASE-TX RJ45 copper interfaces delivered in an IP40 rugged, strong case with redundant power system. Its slim case is suitable for such applications as surveillance system deployments, control management and wireless service in climatically demanding environments with wide temperature range from -40℃ to 80℃.

The LBTR05F series provides the flexibility to all kinds of 10/100Mbps Ethernet Media on RJ-45 port and performs highly stable fiber performance.

The LBTR05F series is packaged in a compact IP40 case that allows either DIN rail or panel mounting to have efficient usage of cabinet space. It provides an integrated power supply with a wide range of voltages for worldwide operation. It also offers dual-redundant, reversible polarity 12V DC to 52V DC power supply inputs for high availability applications requiring dual or backup power inputs.

**Specifications:**

|  |  |
| --- | --- |
| Model No. | **LBTR05F** |
| 10/100BASE-TX Port | 5 port RJ-45 auto-MDI / MDI-X |
| Performance Specification | Bandwidth: 1.6Gbps  Packet Buffer Memory:1Mbit Packet Forwarding Rate:1.2Mpps MAC Address Table: 2K |
| Installation | DIN rail |
| Maximum Frame Size | 9000bytes packet size |
| Flow Control | Back pressure for half duplex, IEEE 802.3x pause frame for full duplex |
| Enclosure | IP40 aluminum housing |
| LED Indicator | Power: Red  Ethernet: Yellow  POE: Green |
| Power Input | 12 to 52V DC redundant power |
| Power Consumption | 3 watts max |
| Surge protection | ±4KV |
| Network Protocols | IEEE802.3 10BASE-T;  IEEE802.3i 10Base-T;  IEEE802.3u;100Base-TX/FX; |
| Network cables | 10BASE-T: Cat3,4,5 UTP(≤100 meter)  100BASE-TX: Cat5 or later UTP(≤100meter)  1000BASE-TX: Cat6 or later UTP(≤100 meter) |
| Industry Standard | FCC CFR47 Part 15,EN55022/CISPR22, Class A  IEC61000-4-2 (ESD): ±8kV (contact), ±12kV (air)  IEC61000-4-3 (RS): 10V/m (80~1000MHz)  IEC61000-4-4 (EFT): Power Port: ±4kV; Data Port: ±2kV  IEC61000-4-5 (Surge): Power Port: ±2kV/DM, ±4kV/CM; Data Port: ±2kV  IEC61000-4-6 (CS): 3V (10kHz-150kHz); 10V (150kHz-80MHz)  IEC61000-4-16 (Common mode conduction): 30V (cont.), 300V (1s) |
| Certification | CE FCC Rohs compliance |
| MTBF | >300,000hours |
| Dimensions (W x D x H) | 118 x 86 x 33.5 mm |
| Weight | Product Weight: 0.36KG  Packing Weight: 0.46KG |
| Working Environment | Working temperature: -40 – 80 degree  Storage temperature: -40 – 80 degree  Relative Humidity: 5%~95 %( no condensation) |
| Warranty | 1-year replacement with new item; 3-years for main parts. |

**Dimensions**

